{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"清单","index":0,"n_rows":75,"n_cols":8,"rows_kept":75,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["南城校区图书馆七楼档案室装修改造项目清单"]
["序号","项目名称","特征描述","单位","数量","综合单价","合价（元）","备注"]
["一","拆除部分"]
[1,"拆除原有砖墙","1.拆除原有内墙200厚","m2",105]
[2,"拆除原有铝合金窗及不锈钢防盗网","1.拆除原有铝合金窗及不锈钢防盗网，并搬运到博5地下室","m2",37.199999999999996]
[3,"铲除原有开裂墙面","1.铲除原有开裂墙面抹灰层","m2",252]
[4,"拆除原有栏杆","1.拆除原有生锈不锈钢栏杆，搬运至博5地下室","m",12]
[5,"拆除原有电气","1.拆除原有灯具、风扇、插座及线管配线","m2",180]
[6,"栏杆底部反坎铲除","1.铲除原有栏杆底部反坎抹灰层，0.2宽0.2高","m",12]
[7,"拆除部分垃圾外运","1.拆除部分垃圾外运","车",5]
["二","装修部分"]
[1,"门洞封堵","1.1.5*4.5门洞封堵,200厚砖墙","m2",6.300000000000001]
[2,"门洞抹灰","1.门洞抹灰.20mm厚砂浆抹灰","m2",12.600000000000001]
[3,"门洞油漆","1.刮腻子遍数:满刮腻子二道,砂纸磨平\n2.油漆品种、刷漆遍数:白色内墙漆一底二面(A级无机涂料)","m2",12.600000000000001]
[4,"新砌砖墙","1.墙体类型:内墙\n2.墙体厚度:200\n3.砌块品种、规格、强度等级:蒸压加气混凝土砌块\n4.砂浆强度等级:水泥砂浆M7.5","m2",{"v":63,"d":"63.00"}]
[5,"新砌墙面挂网","1.墙面挂网","m2",{"v":126,"d":"126.00"}]
[6,"新砌墙面抹灰","1.结合层:刷界刷素水泥浆一道\n2.底层厚度、砂浆配合比:15厚M10抹灰砂浆,分层抹灰\n3.面层厚度、砂浆配合比:5厚M15水泥抹灰砂浆\n","m2",{"v":126,"d":"126.00"}]
[7,"新砌墙面抹灰面油漆","1.刮腻子遍数:满刮腻子二道,砂纸磨平\n2.油漆品种、刷漆遍数:白色内墙漆一底二面(A级无机涂料)","m2",{"v":126,"d":"126.00"}]
[8,"新开门洞","1.新开门洞1.5*2.4含切缝、打墙、门边修复","樘",1]
[9,"预制过梁","1.新做过梁200宽100高，含钢筋、混凝土、模板","m",6.300000000000001]
[10,"新做不锈钢门","1.新做304不锈钢双开门，双面板，不需要做闭门器，门框不锈钢包边","m2",7.199999999999999]
[11,"不锈钢包边","1.门框304不锈钢包边，200mm宽","m",12.6]
[12,"新做木门","1.新做杂物间木门，0.9*2.2","樘",1]
[13,"旧墙面刷防水","1.漏水墙面整墙刷防水2遍","m2",81]
[14,"旧墙面挂网","1.旧墙面挂网","m2",252]
[15,"旧墙面抹灰","1.结合层:刷界刷素水泥浆一道\n2.底层厚度、砂浆配合比:15厚M10抹灰砂浆,分层抹灰\n3.面层厚度、砂浆配合比:5厚M15水泥抹灰砂浆\n","m2",252]
[16,"天花油漆","1.刮腻子遍数:满刮腻子二道,砂纸磨平\n2.油漆品种、刷漆遍数:白色内墙漆一底二面(A级无机涂料)","m2",161.7]
[17,"新做不锈钢栏杆","1.新做304不锈钢栏杆，高度1.05m，最底部横杆离地高度30cm，竖杆间距15cm","m",12]
[18,"栏杆底部反坎重新抹灰","1.栏杆底部反坎抹灰，0.2宽0.2高","m",12]
[19,"栏杆底部反坎重新贴砖","1.栏杆底部反坎贴砖，0.2宽0.2高","m",12]
[20,"窗户胶条翻新","1.原有窗户打胶固定拆除，重新装胶条或打胶，窗户翻新可开窗","m2",55.2]
[21,"栏杆位置开槽","1.栏杆位置开槽做排水槽，就近接入排水管，100*50mm","m",12]
[22,"栏杆位置排水槽抹灰","1.栏杆位置排水槽抹平，就近接入排水管，100*50mm","m",12]
[23,"原有破损瓷砖修补","1.原有800*800瓷砖破损修补，按实际需要修补","m2",20]
[24,"新做踢脚线","1.新做踢脚线，100mm高瓷砖踢脚线","m",105.6]
[25,"新做窗帘盒","1.新做木质窗帘盒","m",12]
[26,"新做铝扣板天花","1.新做600*600mm铝扣板天花","m2",54]
[27,"墙面开孔","1.排气扇管道墙面开孔DN150","个",{"v":2,"d":"2.00"}]
[28,"墙边修补","1.旧墙边修复，水泥砂浆修复抹平，阳角位置","m",{"v":9,"d":"9.00"}]
[29,"砖砌反坎","1.砖砌反坎200宽200高，包含抹灰及贴砖","m",{"v":3,"d":"3.00"}]
[30,"铝合金隔断","1.钢化玻璃铝合金隔断，凤铝牌，12mm钢化玻璃","m2",{"v":19.2,"d":"19.20"}]
[31,"砖砌护墙","1.墙体类型:内墙\n2.墙体厚度:200\n3.砌块品种、规格、强度等级:蒸压加气混凝土砌块\n4.砂浆强度等级:水泥砂浆M7.5","m2",{"v":63.60000000000001,"d":"63.60"}]
[32,"护墙墙面挂网","1.墙面挂网","m2",{"v":63.60000000000001,"d":"63.60"}]
[33,"护墙墙面抹灰","1.结合层:刷界刷素水泥浆一道\n2.底层厚度、砂浆配合比:15厚M10抹灰砂浆,分层抹灰\n3.面层厚度、砂浆配合比:5厚M15水泥抹灰砂浆\n","m2",{"v":63.60000000000001,"d":"63.60"}]
[34,"护墙抹灰面油漆","1.刮腻子遍数:满刮腻子二道,砂纸磨平\n2.油漆品种、刷漆遍数:白色内墙漆一底二面(A级无机涂料)","m2",{"v":63.60000000000001,"d":"63.60"}]
[35,"排水管包管","1.钛晶板包管，0.5*0.5m通高包管，包含预留检查口","m2",{"v":8.4,"d":"8.40"}]
["三","电气部分"]
[1,"平板灯","1.600*600mm天花吊顶平板灯","个",6]
[2,"LED节能防爆灯","1.旧天花新做LED节能防爆灯","个",15]
[3,"LED节能灯","1.杂物间做LED节能灯","个",2]
[4,"电气安装","1.新增线管DN25、配线BV-2.5mm，含网线及网线线管、电话线及电话线线管","m2",{"v":180,"d":"180.00"}]
[5,"新增空调插座","1.新增空调插座，带开关","个",{"v":4,"d":"4.00"}]
[6,"新做配电箱","1.新增配电箱及漏电开关，正泰，每台空调独立开关控制","套",{"v":1,"d":"1.00"}]
[7,"新增排气扇","1.天花吊顶排气扇600*600mm","套",{"v":2,"d":"2.00"}]
[8,"排气扇管道","1.排气扇管道DN100","m",{"v":16,"d":"16.00"}]
[9,"消防感烟探测器改位","1.天花吊顶位置感烟探测器改位","套",{"v":8,"d":"8.00"}]
[10,"插座","1.新增插座","个",{"v":18,"d":"18.00"}]
[11,"网络插座","1.新增网络插座","个",{"v":9,"d":"9.00"}]
[12,"电话插座","1.新增电话插座","个",{"v":3,"d":"3.00"}]
[13,"电子智能锁","1.不锈钢门安装电子智能锁","套",{"v":2,"d":"2.00"}]
[14,"配电房增加控制箱及开关","1.配电房新增控制箱及控制开关3P63A","套",{"v":1,"d":"1.00"}]
[15,"新增主电缆","1.主电缆YJV-5*16mm2","m",{"v":126,"d":"126.00"}]
[16,"新增电缆保护管","1.电缆保护管PC50","m",{"v":126,"d":"126.00"}]
["四","其他"]
[1,"白蚁防治及消杀","1.白蚁防治及消杀","m2",{"v":180,"d":"180.00"}]
[2,"场地保护现有用品搬运","1.原有杂物搬移到指定位置","项",{"v":1,"d":"1.00"}]
[3,"材料二次搬运及电梯保护","1.材料二次搬运及电梯保护","项",{"v":1,"d":"1.00"}]
[4,"卫生清理","1.场地卫生精细保洁","m2",{"v":180,"d":"180.00"}]
[5,"脚手架搭拆费","1.脚手架搭拆费，高度4.5m以内","m2",{"v":180,"d":"180.00"}]
[6,"夜间施工增加费","1.工期紧张，需夜间施工，白天不得影响学生学习","m2",{"v":180,"d":"180.00"}]
[null,"小计"]
["A","文明施工及管理费5%"]
["B","税金9%"]
["C","含税总造价"]
[null,"制表：",null,"审核："]